
Video 1 : Introduction to computer network and ip addresses



Video 2 : Types of Casting, Unicast and Broadcast

BroadCasting -

1. Limited BroadCasting : broadcast to all hosts in same network

Limited broadcast address : 255.255.255.255

1. Directed BroadCasting : broadcast to all hosts in different network

Directed broadcast address : otherhostid.all1’s eg. 20.255.255.255


Video 3 : Subnets, Subnet masking, Routing

Subnetting –


1. Wastageof ip address ( 2 per subnet)
2. For more than one match, go for longest subnet mask eg. Prefer/15 to /12
3. Doesn’t match to any entry goes to default (0.0.0.0 sm 0.0.0.0)

Video 4 : Variable length subnet masking


200.1.2.0 – Three networks of 128,64,64. Other than soln below nid’s can be(0,64,128)



Video 5 : Subnet masking questions



Video 6 : Classless InterDomain Routing



Video 7 : Subnetting, VLSM in CIDR


Based on above Concepts

Video 8 : Prolems on Subnet mask

Should be solved

Video 9 : Supernetting and aggregation

I.Continious, II.Same size, III.First NID/size of block



Video 10 : Delays in CN

1. Transmission Delay = Bits / Bandwidth (time to put data from sender to channel)
2. If Data is given as K, it is 1024, For Bits 1K=1024bits, For BW 1kbps=1000bps
3. Propagation Delay = distance / Speed (time to reach the destination)
4. Speed of optical fibre is 70% of light speed, i.e 0.7\*3\*10pow8 = 2.1\*10pow8
5. Queuing Delay = wait in buffer until picked up from queue
6. Processing Delay = time to process the packet

Video 11 : Flow Control Methods, Stop and Wait

Efficiency = Tt / ( Tt +2\*Tp )

Throughput (Effective Bandwidth / BW Utilization)(in bps) = ( bits / ( Tt + 2\*Tp ) )

= ( ( bits / Bw ) / ( Tt + 2\*Tp ) ) \* Bw = ( Tt / ( Tt +2\*Tp ) ) \* Bw

= Efficiency \* Bandwidth

Final Packet = S&W + TimoutTimer + SeqNo to Data + SeqNo to Ack

Error Probability = p, Total packets sent = n + np + np2 + … = n(1+p+p2+…) = n(1/(1-p))

Video 12 : Capacity of pipe and pipelining

Capacity = Bandwidth \* Propagation Delay (For Full duplex mult by 2)

Thick pipe (more capacity), Stop and wait efficiency is less here

Thin pipe (less capacity), Stop and Wait efficiency is more here

Sliding Window Protocol

Window size = 1 + 2a

Min Seq no = 1 + 2a

Bits reqd = log2( 1 + 2a )

Ws = min ( 1 + 2a , 2powN )

Video 13 : Go Back N